{"text_format":"2","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Estimate for Civil work","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":8,"n_cols":3,"rows_kept":8,"cut":false,"hidden":false,"merged":[[0,0,0,5],[2,2,4,2]]}
["Sarvodaya Parivar Trust funding request"]
[null,null,"Rs"]
[null,"1 Removing old worn out / damaged 40 years old AC sheets roofing as well as old damaged / bent wooden purlins  and replacing by GI precoated  TATA make sheets and by anti - corrosive painted MS Purlins.",{"$f":"'Estimate for Civil work'!F32","v":1019442.5}]
[null,"2 School building is 40 years old load bearing structure which has developed cracks at many places in the wall. Repairs will involve chipping out the cracks and filling them up with SIKA make RBR compound and then refinishing them and painting with cement based paint. "]
[null,"3 the existing Toilet Block is not sufficient for existing No. of students. 12 new toilets will be constructed in the first phase and the  necessary repairs will be carried out inthe existing toilets."]
[null,"Microscopes 2 Nos, Vision 2000",{"$f":"2*28500","v":57000}]
[null,"Camera Coolpix P7800, 2 Nos",{"$f":"27950*2","v":55900}]
[null,"Total",{"$f":"SUM(C3:C7)","v":1132342.5}]

{"sheet":"Estimate for Civil work","index":1,"n_rows":34,"n_cols":6,"rows_kept":34,"cut":false,"hidden":false,"merged":[[0,0,0,5],[1,0,1,5],[6,0,6,5]]}
["LANDMARK DEVELOPERS"]
["16. Kshiteej appt.  First flooor, TITHAL ROAD, VALSAD 396 001"]
[]
[]
[{"$nulls":5},"22.12.2015"]
[]
["ESTIMATE FOR CIVIL WORK FOR SCHOOL BUILDING AT PINDWAL"]
[]
[]
[]
["SR NO","ITEM DESCRIPTION","UNIT","QTY","RATE","AMOUNT"]
[]
[1,"P/L  G.I.  PRECOATED SHEETS  INCLUDING","SQMT",435,415,180525]
[null," REMOVING OF OLD  SHEETS"]
[]
[2,"P/F M.S. STRUCTURAL SUPPORTS INCLUDING ","TONNE",3.45,58000,200100]
[null,"PAINTING WORK"]
[]
[3,"P/L REPAIRING WORK BY DOING  CRACK FILLING ","RMT.",745,125,93125]
[null,"WORK TO WALL STRUCTURE"]
[]
[4,"CIVIL WORK FOR MAKING TOILETS INCLUDING","UNIT",12,38000,456000]
[null,"PLUMBING AND SANITARY FITTINGS AS WELL AS"]
[null,"INLET AND OUTLET LINES"]
[]
[5,"WHITE WASHING AND OIL PAINTING WORK","L.S.",1,60000,60000]
[]
[]
[]
[{"$nulls":5},989750]
[null,null,"ADD 3 % CONTIGENCIES",null,null,29692.5]
[{"$nulls":5},1019442.5]
[]
[null,"                                                                                               TOTAL AMOUNT  SAY Rs.  10,19000.00  ONLY"]

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}